{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["NeverDie Calculator"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"NeverDie Calculator","index":0,"n_rows":16,"n_cols":3,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
["NeverDie® BMS Advanced Series - System Status bits calculator"]
[]
["Enter System Status value here","000001"]
["Then press Calculate button"]
[]
["High Voltage State","AUX Contacts State","AGSR On/Off State"]
["Charge Source Detected","AUX Contacts Error","High Temperature State"]
["NeverDie® Reserve State","Pre-charge Error","Low Temperature State"]
["OptoLoop® Open Circuit","Contactor Flutter","AUX Input 1 State"]
["Reserve Voltage Range","AC Power Present","Charge Disable"]
["Low Voltage State","TSM Charger Present","Overcurrent State"]
["Battery Protection State","TSM Charger Error","not used"]
["Power Off State","Temp Sensor Error","not used"]
[]
["NOTE: This version of the System Status bits calculator applies to NeverDie® BMS version 7.13 and above"]